<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<system name="DE2_70_SOPC">
    <parameter valueString="-2494972993" name="systemHash"/>
    <parameter name="quartusRootDir">c:\altera\72\quartus</parameter>
    <parameter valueString="1193364146623" name="timeStamp"/>
    <parameter valueString="false" name="generateLegacySDK"/>
    <parameter name="bonusData">bonusData 
{
   element timer_stamp
   {
      datum _sortIndex
      {
         value = "6";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element cpu.jtag_debug_module
   {
      datum baseAddress
      {
         value = "4458496";
         type = "long";
      }
   }
   element uart.s1
   {
      datum baseAddress
      {
         value = "4460544";
         type = "long";
      }
   }
   element tristate_bridge.avalon_slave
   {
      datum baseAddress
      {
         value = "0";
         type = "long";
      }
   }
   element timer.s1
   {
      datum baseAddress
      {
         value = "4460576";
         type = "long";
      }
   }
   element lcd
   {
      datum _sortIndex
      {
         value = "12";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element jtag_uart.avalon_jtag_slave
   {
      datum baseAddress
      {
         value = "4460720";
         type = "long";
      }
   }
   element DE2_70_SOPC
   {
   }
   element tristate_bridge
   {
      datum _sortIndex
      {
         value = "10";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element onchip_mem
   {
      datum _sortIndex
      {
         value = "1";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{memorySize=KBytes}";
         type = "String";
      }
   }
   element pll.s1
   {
      datum baseAddress
      {
         value = "4460640";
         type = "long";
      }
   }
   element cpu
   {
      datum _sortIndex
      {
         value = "0";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element clk
   {
   }
   element timer
   {
      datum _sortIndex
      {
         value = "5";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element onchip_mem.s1
   {
      datum baseAddress
      {
         value = "4325376";
         type = "long";
      }
   }
   element sysid
   {
      datum _sortIndex
      {
         value = "8";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element pio_led.s1
   {
      datum baseAddress
      {
         value = "4460688";
         type = "long";
      }
   }
   element pio_led
   {
      datum _sortIndex
      {
         value = "11";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element pll.c1
   {
      datum _clockDomain
      {
         value = "pll_c1_memory";
         type = "String";
      }
   }
   element timer_stamp.s1
   {
      datum baseAddress
      {
         value = "4460608";
         type = "long";
      }
   }
   element pll.c0
   {
      datum _clockDomain
      {
         value = "pll_c0_system";
         type = "String";
      }
   }
   element camera
   {
      datum _sortIndex
      {
         value = "4";
         type = "int";
      }
   }
   element uart
   {
      datum _sortIndex
      {
         value = "3";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element ssram
   {
      datum _sortIndex
      {
         value = "9";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element jtag_uart
   {
      datum _sortIndex
      {
         value = "2";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element lcd.control_slave
   {
      datum baseAddress
      {
         value = "4460704";
         type = "long";
      }
   }
   element camera.s1
   {
      datum baseAddress
      {
         value = "4460672";
         type = "long";
      }
   }
   element sysid.control_slave
   {
      datum baseAddress
      {
         value = "4460728";
         type = "long";
      }
   }
   element pll
   {
      datum _sortIndex
      {
         value = "7";
         type = "int";
      }
      datum megawizard_uipreferences
      {
         value = "{}";
         type = "String";
      }
   }
   element ssram.s1
   {
      datum baseAddress
      {
         value = "2097152";
         type = "long";
      }
   }
}
</parameter>
    <parameter valueString="false" name="hardcopyCompatible"/>
    <parameter valueString="CYCLONEII" name="deviceFamily"/>
    <parameter valueString="false" name="generateLegacySim"/>
    <parameter valueString="DE2_70_D5M_XVGA.qpf" name="projectName"/>
    <parameter valueString="VERILOG" name="hdlLanguage"/>
    <parameter name="projectDirectory">D:\NIOS_II\DE2-70\DE2_70_CAMERA</parameter>
    <module version="7.2" name="clk" kind="clock_source">
        <parameter valueString="true" name="clockFrequencyKnown"/>
        <parameter valueString="50000000" name="clockFrequency"/>
    </module>
    <module version="7.2" name="cpu" kind="altera_nios2">
        <parameter valueString="" name="userDefinedSettings"/>
        <parameter valueString="Automatic" name="setting_branchPredictionType"/>
        <parameter valueString="_10" name="mmu_processIDNumBits"/>
        <parameter valueString="32" name="exceptionOffset"/>
        <parameter valueString="EmbeddedMulFast" name="muldiv_multiplierType"/>
        <parameter valueString="_4096" name="icache_size"/>
        <parameter valueString="_128" name="debug_OCIOnchipTrace"/>
        <parameter valueString="Fast" name="impl"/>
        <parameter valueString="_2" name="mmu_uitlbNumEntries"/>
        <parameter valueString="onchip_mem.s1" name="exceptionSlave"/>
        <parameter valueString="false" name="dcache_omitDataMaster"/>
        <parameter valueString="0" name="mmu_TLBMissExcOffset"/>
        <parameter valueString="false" name="setting_illegalMemAccessDetection"/>
        <parameter valueString="32" name="breakOffset"/>
        <parameter valueString="true" name="debug_embeddedPLL"/>
        <parameter valueString="false" name="setting_debugSimGen"/>
        <parameter valueString="false" name="setting_alwaysBypassDCache"/>
        <parameter valueString="_0" name="icache_numTCIM"/>
        <parameter valueString="false" name="setting_showInternalSettings"/>
        <parameter valueString="false" name="setting_illegalInstructionsTrap"/>
        <parameter valueString="0" name="resetOffset"/>
        <parameter valueString="false" name="setting_bhtIndexPcOnly"/>
        <parameter valueString="true" name="setting_HDLSimCachesCleared"/>
        <parameter valueString="true" name="setting_alwaysEncrypt"/>
        <parameter valueString="false" name="setting_activateModelChecker"/>
        <parameter valueString="_32" name="dcache_lineSize"/>
        <parameter valueString="false" name="setting_allowFullAddressRange"/>
        <parameter valueString="_10" name="mmu_dtlbPtrSz"/>
        <parameter valueString="_2" name="mmu_itlbNumWays"/>
        <parameter valueString="false" name="setting_avalonDebugPortPresent"/>
        <parameter valueString="false" name="cpuReset"/>
        <parameter valueString="true" name="setting_clearXBitsLDNonBypass"/>
        <parameter valueString="_2" name="mmu_dtlbNumWays"/>
        <parameter valueString="onchip_mem.s1" name="resetSlave"/>
        <parameter valueString="_32" name="setting_perfCounterWidth"/>
        <parameter valueString="" name="mmu_TLBMissExcSlave"/>
        <parameter name="breakSlave">cpu.jtag_debug_module</parameter>
        <parameter valueString="false" name="setting_preciseIllegalMemAccessException"/>
        <parameter valueString="Level4" name="debug_level"/>
        <parameter valueString="false" name="muldiv_divider"/>
        <parameter valueString="false" name="dcache_bursts"/>
        <parameter valueString="true" name="setting_activateMonitors"/>
        <parameter valueString="true" name="setting_bit31BypassDCache"/>
        <parameter valueString="Automatic" name="icache_ramBlockType"/>
        <parameter valueString="_8" name="setting_bhtPtrSz"/>
        <parameter valueString="false" name="setting_preciseDivisionErrorException"/>
        <parameter valueString="false" name="setting_preciseSlaveAccessErrorException"/>
        <parameter valueString="false" name="debug_debugReqSignals"/>
        <parameter valueString="_2" name="mmu_udtlbNumEntries"/>
        <parameter valueString="_0" name="dcache_numTCDM"/>
        <parameter valueString="false" name="setting_fullWaveformSignals"/>
        <parameter valueString="false" name="setting_performanceCounter"/>
        <parameter valueString="_10" name="mmu_itlbPtrSz"/>
        <parameter valueString="_2048" name="dcache_size"/>
        <parameter valueString="Automatic" name="dcache_ramBlockType"/>
        <parameter valueString="true" name="setting_activateTrace"/>
        <parameter valueString="false" name="setting_HBreakTest"/>
        <parameter valueString="false" name="setting_exportPCB"/>
        <parameter valueString="false" name="setting_activateTestEndChecker"/>
        <parameter valueString="None" name="icache_burstType"/>
        <parameter valueString="false" name="setting_showUnpublishedSettings"/>
        <parameter valueString="true" name="debug_triggerArming"/>
        <parameter valueString="false" name="mmu_enabled"/>
    </module>
    <module version="7.2" name="onchip_mem" kind="altera_avalon_onchip_memory2">
        <parameter valueString="32" name="dataWidth"/>
        <parameter valueString="false" name="dualPort"/>
        <parameter valueString="true" name="writable"/>
        <parameter valueString="1" name="slave1Latency"/>
        <parameter valueString="true" name="initMemContent"/>
        <parameter valueString="onchip_mem" name="initializationFileName"/>
        <parameter valueString="false" name="useNonDefaultInitFile"/>
        <parameter valueString="false" name="allowInSystemMemoryContentEditor"/>
        <parameter valueString="1" name="slave2Latency"/>
        <parameter valueString="false" name="simAllowMRAMContentsFile"/>
        <parameter valueString="false" name="useShallowMemBlocks"/>
        <parameter valueString="AUTO" name="blockType"/>
        <parameter valueString="NONE" name="instanceID"/>
        <parameter valueString="92160" name="memorySize"/>
    </module>
    <module version="7.2" name="jtag_uart" kind="altera_avalon_jtag_uart">
        <parameter valueString="8" name="readIRQThreshold"/>
        <parameter valueString="" name="simInputCharacterStream"/>
        <parameter valueString="0" name="hubInstanceID"/>
        <parameter valueString="64" name="readBufferDepth"/>
        <parameter valueString="false" name="allowMultipleConnections"/>
        <parameter valueString="64" name="writeBufferDepth"/>
        <parameter valueString="8" name="writeIRQThreshold"/>
        <parameter valueString="false" name="useRegistersForWriteBuffer"/>
        <parameter valueString="false" name="useRegistersForReadBuffer"/>
        <parameter name="simInteractiveOptions">INTERACTIVE_ASCII_OUTPUT</parameter>
    </module>
    <module version="7.2" name="uart" kind="altera_avalon_uart">
        <parameter valueString="115200" name="baud"/>
        <parameter valueString="8" name="dataBits"/>
        <parameter valueString="NONE" name="parity"/>
        <parameter valueString="false" name="simTrueBaud"/>
        <parameter valueString="false" name="useEopRegister"/>
        <parameter valueString="1" name="stopBits"/>
        <parameter valueString="100000000" name="clockRate"/>
        <parameter valueString="false" name="simInteractiveOutputEnable"/>
        <parameter valueString="" name="simCharStream"/>
        <parameter valueString="0.01" name="baudError"/>
        <parameter valueString="true" name="fixedBaud"/>
        <parameter valueString="true" name="useCtsRts"/>
        <parameter valueString="false" name="simInteractiveInputEnable"/>
    </module>
    <module version="1.0" name="camera" kind="CAMERA_IF">
        <parameter valueString="" name="sharedPorts"/>
    </module>
    <module version="7.2" name="timer" kind="altera_avalon_timer">
        <parameter valueString="CUSTOM" name="timerPreset"/>
        <parameter valueString="1.0" name="period"/>
        <parameter valueString="false" name="resetOutput"/>
        <parameter valueString="MSEC" name="periodUnits"/>
        <parameter valueString="false" name="fixedPeriod"/>
        <parameter valueString="false" name="alwaysRun"/>
        <parameter valueString="false" name="timeoutPulseOutput"/>
        <parameter valueString="true" name="snapshot"/>
    </module>
    <module version="7.2" name="timer_stamp" kind="altera_avalon_timer">
        <parameter valueString="CUSTOM" name="timerPreset"/>
        <parameter valueString="1.0" name="period"/>
        <parameter valueString="false" name="resetOutput"/>
        <parameter valueString="MSEC" name="periodUnits"/>
        <parameter valueString="false" name="fixedPeriod"/>
        <parameter valueString="false" name="alwaysRun"/>
        <parameter valueString="false" name="timeoutPulseOutput"/>
        <parameter valueString="true" name="snapshot"/>
    </module>
    <module version="7.2" name="pll" kind="altera_avalon_pll">
        <parameter name="e2">tap e2 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c0">tap c0 mult 2 div 1 phase 0 enabled true inputfreq 50000000 outputfreq 100000000 
</parameter>
        <parameter name="c7">tap c7 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter valueString="Register" name="resetInputPortOption"/>
        <parameter valueString="CYCLONEII" name="deviceFamily"/>
        <parameter valueString="50000000" name="inputClockFrequency"/>
        <parameter valueString="Export" name="lockedOutputPortOption"/>
        <parameter name="e3">tap e3 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c1">tap c1 mult 2 div 1 phase -1806 enabled true inputfreq 50000000 outputfreq 100000000 
</parameter>
        <parameter name="c6">tap c6 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="pllHdl">//  megafunction wizard: %ALTPLL%
//  GENERATION: STANDARD
//  VERSION: WM1.0
//  MODULE: altpll

// ============================================================
// CNX file retrieval info
// ============================================================
// Retrieval info: PRIVATE: ACTIVECLK_CHECK STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH STRING "1.000"
// Retrieval info: PRIVATE: BANDWIDTH_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH_FREQ_UNIT STRING "MHz"
// Retrieval info: PRIVATE: BANDWIDTH_PRESET STRING "Low"
// Retrieval info: PRIVATE: BANDWIDTH_USE_AUTO STRING "1"
// Retrieval info: PRIVATE: BANDWIDTH_USE_CUSTOM STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH_USE_PRESET STRING "0"
// Retrieval info: PRIVATE: CLKBAD_SWITCHOVER_CHECK STRING "0"
// Retrieval info: PRIVATE: CLKLOSS_CHECK STRING "0"
// Retrieval info: PRIVATE: CLKSWITCH_CHECK STRING "0"
// Retrieval info: PRIVATE: CNX_NO_COMPENSATE_RADIO STRING "0"
// Retrieval info: PRIVATE: CREATE_CLKBAD_CHECK STRING "0"
// Retrieval info: PRIVATE: CREATE_INCLK1_CHECK STRING "0"
// Retrieval info: PRIVATE: CUR_DEDICATED_CLK STRING "c0"
// Retrieval info: PRIVATE: CUR_FBIN_CLK STRING "e0"
// Retrieval info: PRIVATE: DEVICE_SPEED_GRADE STRING "Any"
// Retrieval info: PRIVATE: DIV_FACTOR0 NUMERIC "1"
// Retrieval info: PRIVATE: DIV_FACTOR1 NUMERIC "1"
// Retrieval info: PRIVATE: DUTY_CYCLE0 STRING "50.00000000"
// Retrieval info: PRIVATE: DUTY_CYCLE1 STRING "50.00000000"
// Retrieval info: PRIVATE: EXPLICIT_SWITCHOVER_COUNTER STRING "0"
// Retrieval info: PRIVATE: EXT_FEEDBACK_RADIO STRING "0"
// Retrieval info: PRIVATE: GLOCKED_COUNTER_EDIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: GLOCKED_FEATURE_ENABLED STRING "1"
// Retrieval info: PRIVATE: GLOCKED_MODE_CHECK STRING "0"
// Retrieval info: PRIVATE: GLOCK_COUNTER_EDIT NUMERIC "1048575"
// Retrieval info: PRIVATE: HAS_MANUAL_SWITCHOVER STRING "1"
// Retrieval info: PRIVATE: INCLK0_FREQ_EDIT STRING "50.000"
// Retrieval info: PRIVATE: INCLK0_FREQ_UNIT_COMBO STRING "MHz"
// Retrieval info: PRIVATE: INCLK1_FREQ_EDIT STRING "100.000"
// Retrieval info: PRIVATE: INCLK1_FREQ_EDIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: INCLK1_FREQ_UNIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: INCLK1_FREQ_UNIT_COMBO STRING "MHz"
// Retrieval info: PRIVATE: INTENDED_DEVICE_FAMILY STRING "Cyclone II"
// Retrieval info: PRIVATE: INT_FEEDBACK__MODE_RADIO STRING "1"
// Retrieval info: PRIVATE: LOCKED_OUTPUT_CHECK STRING "0"
// Retrieval info: PRIVATE: LONG_SCAN_RADIO STRING "1"
// Retrieval info: PRIVATE: LVDS_MODE_DATA_RATE STRING "Not Available"
// Retrieval info: PRIVATE: LVDS_MODE_DATA_RATE_DIRTY NUMERIC "0"
// Retrieval info: PRIVATE: LVDS_PHASE_SHIFT_UNIT0 STRING "ps"
// Retrieval info: PRIVATE: LVDS_PHASE_SHIFT_UNIT1 STRING "ps"
// Retrieval info: PRIVATE: MIRROR_CLK0 STRING "0"
// Retrieval info: PRIVATE: MIRROR_CLK1 STRING "0"
// Retrieval info: PRIVATE: MULT_FACTOR0 NUMERIC "2"
// Retrieval info: PRIVATE: MULT_FACTOR1 NUMERIC "2"
// Retrieval info: PRIVATE: NORMAL_MODE_RADIO STRING "1"
// Retrieval info: PRIVATE: OUTPUT_FREQ0 STRING "100.00000000"
// Retrieval info: PRIVATE: OUTPUT_FREQ1 STRING "100.00000000"
// Retrieval info: PRIVATE: OUTPUT_FREQ_MODE0 STRING "0"
// Retrieval info: PRIVATE: OUTPUT_FREQ_MODE1 STRING "0"
// Retrieval info: PRIVATE: OUTPUT_FREQ_UNIT0 STRING "MHz"
// Retrieval info: PRIVATE: OUTPUT_FREQ_UNIT1 STRING "MHz"
// Retrieval info: PRIVATE: PHASE_RECONFIG_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: PHASE_RECONFIG_INPUTS_CHECK STRING "0"
// Retrieval info: PRIVATE: PHASE_SHIFT0 STRING "0.00000000"
// Retrieval info: PRIVATE: PHASE_SHIFT1 STRING "-65.00000000"
// Retrieval info: PRIVATE: PHASE_SHIFT_STEP_ENABLED_CHECK STRING "0"
// Retrieval info: PRIVATE: PHASE_SHIFT_UNIT0 STRING "ps"
// Retrieval info: PRIVATE: PHASE_SHIFT_UNIT1 STRING "deg"
// Retrieval info: PRIVATE: PLL_ADVANCED_PARAM_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_ARESET_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_AUTOPLL_CHECK NUMERIC "1"
// Retrieval info: PRIVATE: PLL_ENA_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_ENHPLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_FASTPLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_FBMIMIC_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_LVDS_PLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_PFDENA_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_TARGET_HARCOPY_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PRIMARY_CLK_COMBO STRING "inclk0"
// Retrieval info: PRIVATE: RECONFIG_FILE STRING "altpllpll.mif"
// Retrieval info: PRIVATE: SACN_INPUTS_CHECK STRING "0"
// Retrieval info: PRIVATE: SCAN_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: SELF_RESET_LOCK_LOSS STRING "0"
// Retrieval info: PRIVATE: SHORT_SCAN_RADIO STRING "0"
// Retrieval info: PRIVATE: SPREAD_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: SPREAD_FREQ STRING "50.000"
// Retrieval info: PRIVATE: SPREAD_FREQ_UNIT STRING "KHz"
// Retrieval info: PRIVATE: SPREAD_PERCENT STRING "0.500"
// Retrieval info: PRIVATE: SPREAD_USE STRING "0"
// Retrieval info: PRIVATE: SRC_SYNCH_COMP_RADIO STRING "0"
// Retrieval info: PRIVATE: STICKY_CLK0 STRING "1"
// Retrieval info: PRIVATE: STICKY_CLK1 STRING "1"
// Retrieval info: PRIVATE: SWITCHOVER_COUNT_EDIT NUMERIC "1"
// Retrieval info: PRIVATE: SWITCHOVER_FEATURE_ENABLED STRING "1"
// Retrieval info: PRIVATE: SYNTH_WRAPPER_GEN_POSTFIX STRING "0"
// Retrieval info: PRIVATE: USE_CLK0 STRING "1"
// Retrieval info: PRIVATE: USE_CLK1 STRING "1"
// Retrieval info: PRIVATE: USE_CLKENA0 STRING "0"
// Retrieval info: PRIVATE: USE_CLKENA1 STRING "0"
// Retrieval info: PRIVATE: USE_MIL_SPEED_GRADE NUMERIC "0"
// Retrieval info: PRIVATE: ZERO_DELAY_RADIO STRING "0"
// Retrieval info: LIBRARY: altera_mf altera_mf.altera_mf_components.all
// Retrieval info: CONSTANT: CLK0_DIVIDE_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK0_DUTY_CYCLE NUMERIC "50"
// Retrieval info: CONSTANT: CLK0_MULTIPLY_BY NUMERIC "2"
// Retrieval info: CONSTANT: CLK0_PHASE_SHIFT STRING "0"
// Retrieval info: CONSTANT: CLK1_DIVIDE_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK1_DUTY_CYCLE NUMERIC "50"
// Retrieval info: CONSTANT: CLK1_MULTIPLY_BY NUMERIC "2"
// Retrieval info: CONSTANT: CLK1_PHASE_SHIFT STRING "-1806"
// Retrieval info: CONSTANT: COMPENSATE_CLOCK STRING "CLK0"
// Retrieval info: CONSTANT: INCLK0_INPUT_FREQUENCY NUMERIC "20000"
// Retrieval info: CONSTANT: INTENDED_DEVICE_FAMILY STRING "Cyclone II"
// Retrieval info: CONSTANT: LPM_TYPE STRING "altpll"
// Retrieval info: CONSTANT: OPERATION_MODE STRING "NORMAL"
// Retrieval info: CONSTANT: PORT_ACTIVECLOCK STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_ARESET STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKBAD0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKBAD1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKLOSS STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKSWITCH STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CONFIGUPDATE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_FBIN STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_INCLK0 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_INCLK1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_LOCKED STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PFDENA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PHASECOUNTERSELECT STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PHASEDONE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PHASESTEP STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PHASEUPDOWN STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PLLENA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANACLR STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANCLK STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANCLKENA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDATA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDATAOUT STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDONE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANREAD STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANWRITE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk0 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_clk1 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_clk2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk4 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk5 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena4 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena5 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk3 STRING "PORT_UNUSED"
// Retrieval info: USED_PORT: c0 0 0 0 0 OUTPUT_CLK_EXT VCC "c0"
// Retrieval info: USED_PORT: c1 0 0 0 0 OUTPUT_CLK_EXT VCC "c1"
// Retrieval info: USED_PORT: inclk0 0 0 0 0 INPUT_CLK_EXT GND "inclk0"
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll.v TRUE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll.ppf TRUE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll.inc FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll.cmp FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll.bsf FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll_inst.v FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll_bb.v FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll_waveforms.html FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL altpllpll_wave*.jpg FALSE FALSE
</parameter>
        <parameter name="c9">tap c9 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="e0">tap e0 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c5">tap c5 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c2">tap c2 mult 91 div 250 phase 0 enabled false inputfreq 50000000 outputfreq 18200000 
</parameter>
        <parameter name="e1">tap e1 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c8">tap c8 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter valueString="Register" name="pfdenaInputPortOption"/>
        <parameter name="c4">tap c4 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
        <parameter name="c3">tap c3 mult 1 div 1 phase 0 enabled false inputfreq 0 outputfreq 0 
</parameter>
    </module>
    <module version="7.2" name="sysid" kind="altera_avalon_sysid">
        <parameter valueString="1193364147" name="timestamp"/>
        <parameter valueString="347489346" name="id"/>
    </module>
    <module version="7.2" name="ssram" kind="altera_avalon_cy7c1380_ssram">
        <parameter valueString="" name="sharedPorts"/>
        <parameter valueString="2" name="readLatency"/>
        <parameter valueString="true" name="simMakeModel"/>
        <parameter valueString="2" name="size"/>
    </module>
    <module version="7.2" name="tristate_bridge" kind="altera_avalon_tri_state_bridge">
        <parameter valueString="true" name="registerIncomingSignals"/>
    </module>
    <module version="7.2" name="pio_led" kind="altera_avalon_pio">
        <parameter valueString="RISING" name="edgeType"/>
        <parameter valueString="6" name="width"/>
        <parameter valueString="Output" name="direction"/>
        <parameter valueString="LEVEL" name="irqType"/>
        <parameter valueString="false" name="captureEdge"/>
        <parameter valueString="false" name="simDoTestBenchWiring"/>
        <parameter valueString="false" name="generateIRQ"/>
        <parameter valueString="false" name="bitClearingEdgeCapReg"/>
        <parameter valueString="0" name="simDrivenValue"/>
    </module>
    <module version="7.2" name="lcd" kind="altera_avalon_lcd_16207"/>
    <connection version="7.2" start="cpu.instruction_master" kind="avalon" end="cpu.jtag_debug_module">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00440800" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="cpu.jtag_debug_module">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00440800" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.instruction_master" kind="avalon" end="onchip_mem.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00420000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="onchip_mem.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00420000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="jtag_uart.avalon_jtag_slave">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x004410b0" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.d_irq" kind="interrupt" end="jtag_uart.irq">
        <parameter valueString="0" name="irqNumber"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="uart.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.d_irq" kind="interrupt" end="uart.irq">
        <parameter valueString="1" name="irqNumber"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="camera.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441080" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="timer.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441020" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.d_irq" kind="interrupt" end="timer.irq">
        <parameter valueString="2" name="irqNumber"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="timer_stamp.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441040" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.d_irq" kind="interrupt" end="timer_stamp.irq">
        <parameter valueString="3" name="irqNumber"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="pll.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441060" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="clk.clk" kind="clock" end="pll.inclk0"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="cpu.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="onchip_mem.clk1"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="jtag_uart.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="uart.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="timer.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="timer_stamp.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="sysid.clk"/>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="sysid.control_slave">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x004410b8" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="pll.c0" kind="clock" end="ssram.clk"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="tristate_bridge.clk"/>
    <connection version="7.2" start="cpu.instruction_master" kind="avalon" end="tristate_bridge.avalon_slave">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x0000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="tristate_bridge.avalon_slave">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x0000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="tristate_bridge.tristate_master" kind="avalon_tristate" end="ssram.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00200000" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="pll.c0" kind="clock" end="camera.s1_clock"/>
    <connection version="7.2" start="pll.c0" kind="clock" end="pio_led.clk"/>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="pio_led.s1">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x00441090" name="baseAddress"/>
    </connection>
    <connection version="7.2" start="pll.c0" kind="clock" end="lcd.clk"/>
    <connection version="7.2" start="cpu.data_master" kind="avalon" end="lcd.control_slave">
        <parameter valueString="1" name="arbitrationPriority"/>
        <parameter valueString="0x004410a0" name="baseAddress"/>
    </connection>
</system>

